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DS-3WAP5212-EI is an indoor 802.11ac AP product with dual-frequency four-flow design, which meets the wireless coverage requirements of small, medium and micro enterprises

	· 1 × Gigabit PoE in port,1 × Gigabit RJ45 port

	· 802.11ac Wave 2 1200 Mbps

	· Auto RF Optimization

	· Wide Signal Coverage

	· Reliable Wi-Fi Connection

	· Outstanding Wall Penetration
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	· Specification

	General

	Net Weight
	0.36 kg (0.79 lb)

	Gross Weight
	0.6 kg (1.32 lb)

	Installation Mode
	Ceiling Mounting

	Working Temperature
	0°C to 40°C (32°F to 104°F)

	Working Humidity
	10% to 90% (no condensation)

	Storage Temperature
	-40°C to 70°C (-40°F to 158°F)

	Storage Humidity
	5% to 95% (no condensation)

	Product Dimensions (W × H × D)
	Ø220 mm × 49.7 mm (excluding bracket）

	Packing List
	1200 M Access Point × 1, Screw Pack × 1, Installation bracket × 1, Quick Start Guide × 1, Regulatory Compliance and Safety Information × 1

	Power Supply Method
	DC power supply: 12 V, 1.5 A;
PoE power supply: IEEE 802.3at;

	Max. Power Consumption
	18 W

	Wireless Parameter

	Wireless Speed
	Max: 1167 Mbps;
2.4G: 300 Mbps;
5G: 867 Mbps;

	Wireless Standard
	Wi-Fi 5

	Working Frequency Band
	Radio 1: 5G (11a/n/ac);
Radio 2: 2.4G (11b/g/n);

	Recommended Coverage Range
	Recommended Coverage Range: 140 m², the radius in an open environment is 25 meters.
Note: The signal coverage range is greatly affected by the environment. For example, walls, glass doors, and other obstacles will affect the signal coverage. The above - mentioned values are for reference only.

	Max. Number of Connected Clients
	128

	Bandwidth
	2.4G: Auto/20/40 MHz;
5G: Auto/20/40/80 MHz;

	Recommended Number of Connected Clients
	80

	Transmitting Power
	2.4G: Combined power: 28 dBm;
5G: Combined power: 28 dBm;
Note: The actual transmission power varies according to regulations in different countries and regions;

	Spatial Streams
	2.4G: 2 × 2, MU-MIMO
5G: 2 × 2, MU-MIMO

	Wireless Security
	WPA2-PSK, WPA-WPA2-PSK

	Antenna Type
	Built-in omnidirectional antennas

	Antenna Gain
	2.4 GHz: 3.5 dBi
5 GHz: 4.5 dBi

	Hardware Specifications

	Ports
	1 × Gigabit PoE in port, 1 × Gigabit RJ45 port

	RESET
	1 × Reset hole

	Software Specifications

	Max. Number of Wireless SSIDs
	7

	Internet Access Mode
	DHCP,Static

	VLAN ID Range
	1~4000

	Max. Number of VLANs
	8

	Software Features

	Operation Mode
	AP mode (default);
Routing mode;

	Wireless Management
	Support wireless configuration;
Support RF configuration;
Support Health Mode;
Support guest SSID;
Support wireless roaming;
Support wireless optimization;
Support wireless SSID speed limit;
Support wireless RF speed limit;
Support wireless intelligent speed limit;
Support wireless terminal speed limit;
Support weak signal access control;
Support weak signal to kick offline;
Support roaming sensitivity adjustment;
Support wireless access control;
Support wireless terminal association;

	Interface
	Support uplink port VLAN;
Support MAC address modification;
Support LAN configuration;
Support Port VLAN;

	IP Services
	Support DHCP Client;
Supports DHCP Server;
Support LLDP;
Support SADP;

	Service and Support
	Support NAT Traversal;
Support Audit Log;
Support Fault Diagnosis;
Support Fault Alarm;
Support One-Click Fault Collection;
Support Network Diagnostic Tools;
Support SSH;
Support Cloud Service Diagnosis;
Support Local Upgrade;
Support Online Upgrade;
Support Cloud Service;
Support App Management;

	Approval

	EMC
	CE-EMC (EN 55032:2015/A1:2020 EN 55035:2017/A11:2020 EN IEC 61000-3-2:2019/A2:2024 EN 61000-3-3:2013/A2:2021 EN 50130-4:2011/A1:2014)

	Safety
	CB (IEC 62368-1: 2018), CE-LVD (EN 62368-1:2014/A11:2017)

	Chemistry
	CE-RoHS (2011/65/EU), WEEE (2012/19/EU), Reach (Regulation (EC) No.1907/2006)

	Radio
	EN 300 328, EN 300 440, EN 301 893, EN 301 489-1, EN 301 489-3, EN 301 489-17, EN 61000-3-3: 2013+ A1:2019+A2: 2021, EN IEC 61000-3-2: 2019+A1: 2021+A2: 2024, EN IEC 62311: 2020



	· Available Model
DS-3WAP5212-EI
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	· Dimension
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